Liberty Christian School

LOCATION: Dallas, TX

ARCHITECT: F-J L-C & Associates ([www.franzarchitects.com](http://www.franzarchitects.com) )

GENERAL CONTRACTOR: Joeris General Contractors

INSTALLER: Roof Management Services

BERRIDGE DETAILS:

PANEL: Deep Deck

COLOR: Sierra Tan

APPLICATION: Wall

PANEL: R Panel

COLOR: Sierra Tan

APPLICATION: Wall

CATEGORY: K-12

Liberty Christian School was founded in 1983 by Dr. Rodney and Judy Haire with the vision of a providing a preparatory school in a Christian environment thus providing an excellent education with a strong biblical emphasis. Originally located in Denton, Texas the school was moved to Argyle, Texas in 2005. Berridge Manufacturing Company’s Deep Deck Panel and R Panel were used in the light, neutral color choice of Sierra Tan on the exterior of the building. Ideal for East Texas weather, both panels are UL-90 wind resistance rated and UL-790 fire resistance rated. Joeris General Contractors and Roofing Management Services installed the Deep Deck Panel horizontally along the outside walls, while the R Panel were installed vertically on the walls above them. This new larger school now serves 1,300 students and is built to accommodate the rapidly growing school while providing them with a maintenance free building for years to come.