The Venue at The Ballpark

LOCATION: Birmingham, AL

ROOFING INSTALLER: Quality Architect Metal & Roofing

ARCHITECT: BOKA Powell

Material: 137 squares of double rib panel and 16,600 squares of flat sheet (5v crimp)

Color: Acrylic-Coated Galvalume®

Category: Multi-Family

The Venue at The Ballpark is located in Birmingham, AL. This complex features stylish, upscale apartments, extensive amenities and courtyards overlooking Regions Field, providing the best in downtown living.

Designed by BOKA Powell, the modern apartment complex used Berridge Manufacturing’s Double Rib Panel in Acrylic-Coated Galvalume®. Double Rib is typically used for roof applications. In this instance, a non-traditional application was chosen for Double Rib. The 137 squares of Double Rib were installed by Quality Architectural Metal & Roofing on the exterior walls creating a nice contrasting pattern and color combination to the other painted exterior walls. Double Rib is UL-90 wind resistance rated and UL-2218 impact resistance rated. Double Rib is also Florida Product approved making it a good choice for coastal communities.